|  |
| --- |
| Request for Empties / Delivery Note V6.4 |

Send the request for empties to: VTCR.Leitstand-Leergut@voith.com

|  |  |
| --- | --- |
| Ordering date |  |
|  | |
| Collection of empties by | |
| External forwarder |  |
| Self-dealing |  |

|  |  |
| --- | --- |
| Request for empties by | |
| Company |  |
| Person in charge |  |
| Delivery address |  |
| Phone |  |
| E-mail |  |

|  |
| --- |
| Provision of empties by |
| J.M. Voith SE & Co. KG |
| Division Turbo – Crailsheim Location |
| Voithstraße 1, D - 74564 Crailsheim |
| Control Center - Incoming Goods Dept. |
| Phone: +49 7951 32 1844 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | Pallets\* | | | | | | | | | | |
| Pool No. | Designation | | | SAP No. | Dimensions (mm) | Tare weight (kg) | Max. carrying capacity | Rounding value (packing unit) | Loading aids | Current stock - supplier |  | Order quantity (off) nominal qty. | Staging quantity (off)  Actual quantity |
| 1.1.1 | Voith mesh box pallet | | | TCR.09215903 | 1230 x 1030 x 820 | 65 | 1,000 kg | 1 | - |  |  |  |  |
| 1.1.2 | Voith industrial pallet | | | 210.00145700 | 1200 x 1000 x 130 | 37 | 1,000 kg | 1 | - |  |  |  |  |
| 1.1.3 | Voith special pallet | | | 210.00167600 | 1400 x 1400 x 220 | 65 | 4,000 kg | 1 | - |  |  |  |  |
| 1.1.4 | Voith special pallet | | | 210.00167700 | 1800 x 1800 x 220 | 115 | 10,000 kg | 1 | - |  |  |  |  |
| 1.1.5 | Voith special pallet | | | 210.00167800 | 2100 x 2500 x 220 | 175 | 10,000 kg | 1 | - |  |  |  |  |
| 1.1.6 | Voith special pallet | | | 210.00287310 | 830 x 630 x 130 | 10 | 500 kg | 20 | - |  |  |  |  |
| 1.1.7 | Voith special pallet K1 | | | 190.01659910 | 1200 x 1200 x 220 | 168 | 5000 kg | 1 | - |  |  |  |  |
| 1.1.8 | Voith wave pallet K2 | | | 190.01660010 | 2600 x 800 | 208 | 10,000 kg | 1 | - |  |  |  |  |
| 1.1.9 | Voith special pallet K3 | | | 190.01660110 | 1700 x 800 | 141 | 5000 kg | 1 | - |  |  |  |  |
| 1.1.10 | Voith special pallet K4 | | | 190.01678710 | 2600 x 1400 | 395 | 10,000 kg | 1 | - |  |  |  |  |
| 1.1.11 | Voith special pallet K5 | | | 190.01799110 | 2100 x 800 x | 175 | 5000 kg | 1 | - |  |  |  |  |
| 1.1.12 | Voith flat pallet TB1 | | | 190.01664510 | 1700 x 800 x 260 | 80 | 5000 kg | 1 | - |  |  |  |  |
| 1.1.13 | Voith flat pallet TB2 | | | 190.01664610 | 2600 x 800 x 260 | 95 | 10,000 kg | 1 |  |  |  |  |  |

**\* = Europool flat pallets are exchanged via freight forwarder.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | Small load carriers\* | | | | | | | | | | | | | | | |
| Pool No. | Designation | | | SAP No. | Dimensions (mm) | | | Tare weight (kg) | | Max. carrying capacity | | Rounding value (packing unit) | Loading aids | Current stock - supplier |  | Order quantity (off) nominal qty. | Staging quantity (off)  Actual quantity | |
| 2.1 | Small load carrier 2120 | | | 210.00176200 | 200 x 150 x 120 | | | 0.26 | | 15 kg | | 128 | Europool flat pallet |  |  |  |  | |
| 2.2 | Small load carrier 3120 | | | 210.00176300 | 300 x 200 x 120 | | | 0.56 | | 15 kg | | 32 | Europool flat pallet |  |  |  |  | |
| 2.3 | Small load carrier 4120 | | | 210.00176400 | 400 x 300 x 120 | | | 1.0 | | 15 kg | | 24 | Europool flat pallet |  |  |  |  | |
| 2.4 | Small load carrier 4170 | | | 210.00176500 | 400 x 300 x 170 | | | 1.32 | | 15 kg | | 24 | Europool flat pallet |  |  |  |  | |
| 2.5 | Small load carrier 4220 | | | 210.00176600 | 400 x 300 x 220 | | | 1.56 | | 15 kg | | 24 | Europool flat pallet |  |  |  |  | |
| 2.6 | Small load carrier 6120 | | | 210.00176700 | 600 x 400 x 120 | | | 1.72 | | 15 kg | | 16 | Europool flat pallet |  |  |  |  | |
|  | |  |  | | | | | | | | | | | | | | | |
|  | |  | Small load carrier with foam insert\* | | | | | | | | | | | | | | | |
| Pool No. | Designation | | | SAP No. | | Dimensions (mm) | Tare weight (kg) | | Max. carrying capacity | | Rounding value (packing unit) | | Loading aids | Current stock - supplier |  | Order quantity (off) nominal qty. | | Staging quantity (off)  Actual quantity |
| 2.7 | Small load carrier 3120 (28 boreholes) | | | 210.00333910 | | 300 x 200 x 120 25 x 25 | 0.56 | | 15 kg | | 32 | | Europool flat pallet |  |  |  | |  |
| 2.8 | Small load carrier 3120 (20 boreholes) | | | 210.00391310 | | 300 x 200 x 120 25 x 25 | 0.56 | | 15 kg | | 32 | | Europool flat pallet |  |  |  | |  |

**\* = Europool flat pallets are exchanged via freight forwarder.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | Stacking frame\* | | | | | | | | | | | |
| Pool No. | Designation | | | SAP No. | Dimensions (mm) | Tare weight (kg) | Max. carrying capacity | Rounding value (packing unit) | Loading aids | Current stock - supplier |  | Order quantity (off) nominal qty. | Staging quantity (off)  Actual quantity |
| 3.1 | Stacking frame  Europool flat pallet | | | TCR.09216112 | 1200 x 800 x 200 | 10 |  | 20 | Europool flat pallet |  |  |  |  |
| 3.2 | Stacking frame  Voith flat pallet | | | 210.00162900 | 1200 x 1000 x 200 | 10 |  | 20 | VC industrial pallet |  |  |  |  |
| 3.3 | Stacking frame  Voith special pallet | | | 210.00391410 | 800 x 600 x 200 | 10 |  | 20 | Europool flat pallet |  |  |  |  |
|  | |  |  | | | | | | | | | | |
|  | |  | Wave timbers\* | | | | | | | | | | |
| Pool No. | Designation | | | SAP No. | Dimensions (mm) | Tare weight (kg) | Max. carrying capacity | Rounding value (packing unit) | Loading aids | Current stock - supplier |  | Order quantity (off) nominal qty. | Staging quantity (off)  Actual quantity |
| 4.1 | Wave timbers - 1 notches | | | TCR.09215933 | 400 x 120 x 140 | 2 |  | 40 | Europool flat pallet |  |  |  |  |
| 4.2 | Wave timbers - 1 notches | | | 210.00292510 | 750 x 240 x 350 | 32.5 |  | 1 | Europool flat pallet |  |  |  |  |
| 4.3 | Wave timbers - 3 notches | | | TCR.09215936 | 750 x 100 x 80 | 3.5 |  | 30 | Europool flat pallet |  |  |  |  |
| 4.4 | Wave timbers - 4 notches | | | TCR.09215930 | 900 x 140 x 160 | 8 |  | 30 | Europool flat pallet |  |  |  |  |
| 4.5 | Wave timbers - 6 notches | | | 210.00181400 | 940 x 100 x 120 | 6.5 |  | 30 | Europool flat pallet |  |  |  |  |

**\* = Europool flat pallets are exchanged via freight forwarder.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  | Accessories | | | | | | | | | | |
| Pool No. | Designation | | | SAP No. | Dimensions (mm) | Tare weight (kg) | Max. carrying capacity | Rounding value (packing unit) | Loading aids | Current stock - supplier |  | Order quantity (off) nominal qty. | Staging quantity (off)  Actual quantity |
| 5.1 | Stacking corners for stacking frame | | | 210.00180700 | 100 x 100 x 100 | 0.1 |  | 20 | Bag |  |  |  |  |
| 5.2 | Plug-in strips for stacking frame | | | 210.00090100 | 1150 x 180 x 15 | 1.5 |  | 45 | Europool flat pallet |  |  |  |  |
| 210.00090000 | 950 x 180 x 15 | 1.0 |  | 45 |  |  |  |  |
|  |  | | | 210.00588310 | 750 x 180 x 15 | 1.0 |  | 45 |  |  |  |  |  |
| 5.3 | Intermediate layer  Cardboard | | | TCR.09215914 | 700 x 450 | 0.85 |  | 640 | Europool flat pallet |  |  |  |  |
| TCR.09216186 | 1130 x 950 | 2.16 |  | 450 |  |  |  |  |
| 190.01245610 | 1150 x 750 | 2.32 |  | 500 |  |  |  |  |
| 5.4 | Intermediate layer  Plywood | | | 210.00234801 | 1130 x 950 x 10 | 9.5 |  | 40 | VC wire box |  |  |  |  |
| 5.5 | End cover - small load carrier | | | 210.00226500 | 1208 x 808 x 10 | 6.1 |  | 1 | Europool flat pallet |  |  |  |  |
| 5.6 | End cover – small load  Carrier | | | 210.00653310 | 1200 x 1000 x 10 | 8.2 |  | 1 | Voith industrial palette |  |  |  |  |
| 5.7 | Wire-flap bag | | | 210.00407310 | For DIN A4 | 0.1 |  | 100 | Cardboard box |  |  |  |  |